Ricoh Pro VC20000

Not available in US Market There are 3 versions in the Ricoh Pro VC20000 Series: the 75 metres per minute, 600 x 600 dpi mono Ricoh Pro V20000, the 150mpm, 600 x 600 dpi mono Ricoh Pro™ V20100 and the 75mpm, 600 x 600 dpi CMYK Ricoh Pro™ VC20000.

**Product Family:** Pro VC



Productivity

|  |  |
| --- | --- |
| **Speed Reported** |  |
| **FPM Reported** | 225 |
| **IPM Reported** | 500 |
| **Duty Cycle Reported** |  |

Digital Front End

|  |  |
| --- | --- |
| **Controller Options** | TotalFlow R600A |
| **Print Streams** | PDF, Postscript, IPDS, JDF |

Imaging System

|  |  |
| --- | --- |
| **Ink Type** | Aqueous Pigment |
| **Ink Description** |  |
| **Ink Options** | CMYK |
| **Bonding Agent** | not-available |
| **Primer/Precoat** | optional |
| **Drying Methods** |  |
| **Head Technology** | Piezoelectric Drop-on-Demand |
| **Head Manufacturer** | Seiko Epson |
| **Heads Per Engine** | Not Reported |
| **Colors** | 4 |
| **Droplet Size** | Not Reported |
| **Gray levels** | 4 |
| **Resolutions** | 600x600 |

Paper & Media

|  |  |
| --- | --- |
| **Paper Feed** | Roll |
| **Paper Output** | Roll, Sheet, Fold |
| **Minimum Web Width** | Pending Verification |
| **Maximum Web Width** | Pending Verification |
| **Maximum Print Width Simplex** | Pending Verification |
| **Maximum Print Width Duplex** | Pending Verification |
| **Minimum Thickness** | GSM |
| **Maximum Thickness** | GSM |
| **Paper Types** |  |
| **Specialty Media** | Not Reported |

Market Segments

|  |  |
| --- | --- |
| **Manufacturer Segment Notes** | Transactional, Direct Mail |
| **Applications Segments** | Direct Marketing – Postcards & High Color Direct Advertising Direct Marketing – Self Mailers Traditional Transaction Print Transitional Mail |

Configuration

|  |  |
| --- | --- |
| **Layout Configuration** | I, |
| **Print Engines** | 2 |
| **Print Sides** | Duplex |
| **Power Consumption** | Not Reported |
| **Footprint:** | Not Reported |
| **Noise:** | Not Reported |
| **Weight:** | Not Reported |
| **Humidity Range:** | Not Reported |
| **Temperature Range:** | Not Reported |